**Background**

On April 19, 2022, the Maryland Department of the Environment (MDE) began monitoring Back River (Baltimore County) in the vicinity of where the Back River Wastewater Treatment Plant (WWTP) outfall discharges into the river. The purpose of the sampling to understand how WWTP performance problems may be impacting water quality. Bacterial (*Enterococcus* and *E. Coli*) sampling is conducted weekly at four sites (Figure 1).

A screenshot of a computer

Description automatically generated with low confidence

MDE\_BRB\_3

MDE\_BRB\_2

MDE\_BRB\_1

MDE\_BRB\_4

Figure 1: MDE\_BRB\_1 is 500 feet upriver from the outfall; MDE\_BRB\_2 is at the outfall; MDE\_BRB\_3 is 50 feet downriver from the outfall; and, MDE\_BRB\_4 is 600 downriver from the outfall.

The analytical method used can detect the following species of Enterococci.

1. faecalis
2. faecium
3. avium
4. gallinarum
5. casseliflavus
6. durans

MDE provides guidance for the [County Recreational Water Quality Monitoring and Notification Program](https://mde.maryland.gov/programs/Water/Beaches/Documents/MDBEACHrev2020.pdf), which is adapted from the U.S. Environmental Protection Agency (EPA) National Beach Guidance. While this sampling area is not a designated beach, State guidance for beaches can assist in the interpretation of the monitoring results.

As described in the MDE guidance, the purpose of recreational water quality monitoring for bacteria contamination is to inform management actions that reduce the incidence of human illness that arises from contamination of recreational water areas, in particular waters where water contact includes full submersion (swimming). The purpose of water quality indicator testing is to measure the concentration of a bacterial indicator species that are not necessarily a pathogen but whose levels are associated with fecal indicator bacteria and human illness derived from EPA epidemiological studies at beaches. High levels of fecal indicator bacteria suggest water contamination with human or animal fecal matter and resulting potential risk to human health due to the potential for human pathogens to be present.

The guidance includes a Beach Action Level (BAL) that is used to inform beach notifications (also see [COMAR 26.08.09.01](http://www.dsd.state.md.us/comar/comarhtml/26/26.08.09.01.htm)). For example, with designated beaches, if sample results report an indicator organism density above the BAL, then the county should issue a public notification for a beach advisory. If subsequent sampling results in indicator densities below the BAL, then advisories can be lifted. The Beach Action Value for *Enterococci* is 104 Most Probable Number (MPN)/100 milliliters (mL), and the Beach Action Value for *E. Coli* is 235 MPN/100 mL.

The Back River WWTP National Pollutant Discharge Elimination System (NPDES) Permit has a monthly geometric mean permit limit of 126 MPN/100 ml for *E. coli.*, which is consistent with Maryland Surface Water Quality Criteria ([26.08.02.03-3](http://www.dsd.state.md.us/comar/comarhtml/26/26.08.02.03-3.htm)). The monthly geometric mean permit limit is assessed using multiple samples collected over a 30-day monitoring period.

**Monitoring Results**

Bacterial indicator monitoring results for both *Enterococci* (Figure 1) and *E. Coli* (Figure 2) show wide fluctuation in values, with the highest values observed when monitoring occurs within 48 hours of a significant rain event. Sampling events on April 19, May 9 and May 24 all occurred after rain events of 1.22-inches, 2.32-inches, and 0.91-inches, respectively. Data at every station sampled after these rain events exceeded both the BAL for *Enterococci* and the WWTP permit limit for *E. Coli*. Rain events were determined from the [National Atmospheric Administration Data](https://www.ncdc.noaa.gov/cdo-web/datasets/GHCND/stations/GHCND:USW00093721/detail) at Baltimore Washington International Airport.

Sampling dates (April 27, May 4 and May 9) that were not preceded by significant rain show lower *Enterococci* and *E. Coli* values, and generally do not exceed either the BAL or WWTP permit limit, respectively. Outside of wet and dry weather influence on bacteria indicator concentrations, there are no other clear trends either at or between sampling stations. This may be due to multiple bacterial sources in the larger Back River watershed, tidal influences on water quality, and natural variability in bacteria concentrations.

Chart, bar chart

Description automatically generated

Beach Action Value 104

Figure 1: *Enterococci sampling results from Back River in the vicinity of the WWTP outfall.*

Chart, bar chart

Description automatically generated

WWTP Permit Limit 126

Figure 2: *E. Coli sampling results from Back River in the vicinity of the WWTP outfall.*